MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**ECHELON PAVING FOR JOB NUMBER 131656**

TRV:LCP 1 of 1 APPR:NDM:KPK:04-12-21

**a. Description.** This work consists of constructing a longitudinal construction joint by echelon paving where designated on the plans. Ensure all work is completed in accordance with the standard specifications, except as modified herein.

**b. Materials.** None specified.

**c. Construction.** Form the longitudinal construction joint by multiple pavers operating in echelon. Ensure the distance between the pavers is no more than 300 feet. The screed of the following paver will be set to match the grade or thickness of the unrolled edge of the adjacent mat placed. No raking will be allowed to match thicknesses. The rollers compacting the mix behind the lead paver is to stay 6 inches away from the free edge of the mat on the side toward the adjacent paver. Once the mix from the adjacent paver is placed against the uncompacted edge of the mix from the lead paver, the rollers compacting the next lane will be employed to compact the mix on both sides of the joint. At the end of the day the paved mat from the multiple pavers must end at the same point.

**d. Measurement and Payment.** Separate payment will not be made for echelon paving. The cost of this work will be included in the prices bid for other items of work.