MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**TEMPORARY SAFETY RAIL**

BRG:AJM 1 of 1 APPR:JLD:SCK:06-21-21

**a. Description.** This work consists of erecting railing components and supports at various locations as designated on the plans and removing the railing components when no longer needed. Ensure erection is as shown on the plans and specified herein.

**b. Materials.** Furnish rails, posts, and fittings in accordance with subsections 706.02 and 707.02 of the Standard Specification for Construction. Furnish Grade 3500 concrete for post foundations. Galvanizing or other coating is not required for steel railing components.

**c. Construction.** Perform work in accordance with section 711 of the Standard Specifications for Construction. Set the railing to the required levels and lines, with members plumb and true to line. Embed posts in the ground or attach to existing steel in accordance with details on the plans.

**d. Measurement and Payment.** The complete work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Temp Safety Rail. Foot

**Temp Safety Rail** will be measured based on plan quantity or from revised dimensions authorized by the Engineer. No compensation will be made to the Contractor for surplus materials. Payment includes all costs associated with surface preparation and furnishing and placing all materials, labor, equipment necessary to complete this item as shown on the plans and specified herein.