MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**OUT OF SERVICE PIPE, REMOVE**

MTP:JTK 1 of 2 APPR:DMG:NJM:07-21-22

**a. Description.** This work consists of the removal and disposal of 2-inch, 4-inch and 6-inch steel “out of service” gas mains and oil pipelines which conflict with the proposed work.

**b. Materials.** Furnish materials in accordance with the following sections of the Standard Specifications for Construction:

Granular Material Class III 902

Masonry Units 913

Concrete, Grade 3000 1004

Mortar, Type R-2 1005

**c. Construction.** Perform the work in accordance with section 203 of the Standard Specifications for Construction.

Remove sections of “out of service” gas mains and oil pipelines that conflict with the proposed work. Remove to the limits of excavation as directed by the Engineer. Dispose of the removed material in accordance with subsection 205.03.P of the Standard Specifications for Construction.

Bulkhead the gas mains and oil pipelines at the limits of removal in accordance with subsection 402.03.E of the Standard Specifications for Construction.

Backfill excavated areas resulting from the pipeline removal in accordance with subsection 204.03.C of the Standard Specifications for Construction.

Notify all affected companies once a gas main or oil pipeline is uncovered and found to conflict with the proposed work. The owner of the utility must verify if the pipeline is “active” or “out of service” prior to any removal work. Under no circumstance is a gas main or oil pipeline to be removed without this verification.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Out of Serv Pipe, Rem, \_\_ inch Foot

**Out of Serv Pipe, Rem, \_\_ inch** includes excavating, removing, bulkheading, backfilling, and disposing of the material as described and will be measured by the foot of gas main or oil pipeline steel pipe removed.

The removal of non-metallic “out of service” gas mains less than 12 inches in diameter will not be paid for separately but will be included in other items of work.