MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**LANDSCAPE EDGING, ALUM**

COL:JWS 1 of 1 APPR:NMA:JN:04-08-22

**a.** **Description.** This work consists of furnishing and installing aluminum landscape edging as shown on the plans, in accordance with the standard specifications and as directed by the Engineer.

**b. Materials.** Conform to the following requirements:

1. Aluminum, mill finish.

2. Height. 4 inches.

3. Thickness. 3/16 inch.

4. Length. 8 or 16 feet.

5. Stakes. Aluminum 3/16 inch thick by 12 inches long or manufacturer’s standard.

6. Acceptable manufacturers.

A. Permaloc Corporation, Holland, MI 49424: [www.permaloc.com](http://www.permaloc.com)

B. Sure-loc Edging Corporation, Holland, MI 49423: [www.surelocedging.com](http://www.surelocedging.com)

C. Curv-rite Aluminum Edgings, Wayland, MI 49348: [www.curv-rite.com](http://www.curv-rite.com)

**c. Construction.** Install in locations indicated on plans and in accordance with manufacturer's printed instructions.

1. Curved sections. Smooth, without waves or kinks.

2. Straight sections. True to line, without waves or kinks.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Landscape Edging, Alum Foot