MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**DECORATIVE FENCE GATE**

MTP:JTK 1 of 1 APPR:DMG:YGQ:09-01-22

**a. Description.** This work consists of furnishing and installing a decorative sliding fence gate system at the location shown on the plans. This includes any excavation, backfilling, and disposal of unsuitable materials.

**b. Materials.** Furnish a cantilevered sliding fence gate system complete with posts, post caps, and gate hardware.

1. Manufacturer.

Ameristar Perimeter Security USA, Inc.

1555 N. Mingo Road, Tulsa, OK 74116

Phone: (888) 333-3422

Email: AmeristarRegion2@assaabloy.com

Website: <http://www.ameristarperimeter.com>

2. Fence Gate System. Ameristar TransPort II Industrial Cantilever Gate, black coated aluminum Majestic Style, 60 inch height, for 27 foot opening (item number 2TMB06027S).

Furnish concrete Grade 3000 or Grade 3500 for post footings in accordance with section 1004 of the Standard Specifications for Construction.

Submit fence specifications, color samples and shop drawings (in PDF) to the Engineer for approval a minimum of 14 calendar days prior to ordering any materials. Do not order any materials until approval of specifications, color and shop drawings is received from the Engineer.

**c. Construction.** Install fence gate at the location shown on the plans. Install fence gate plumb and level with respect to the adjacent fence posts and panels. Erect fence gate system as recommended by the manufacturer and in accordance with section 808 of the Standard Specifications for Construction.

Ensure the manufacturer of the approved fence system furnishes on-site technical assistance as necessary during installation.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Decorative Fence Gate, 27 Foot Each