MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**HANDHOLE, ROUND, COMMUNICATION**

SUP:JJJ 1 of 1 APPR:BMB:EG:05-28-21

**a. Description.** This work consists of constructing a round communication handhole and furnishing hardware, connectors, fittings.

**b. Materials.** Furnish materials in accordance with section 918 of the Standard Specifications for Construction.

**c. Construction.** Construct the handhole per section 818 of the Standard Specification for Construction.

1. Determine the final location of the handhole based on actual field conditions at the time of construction to ensure no conflicts exist with other systems being installed or with existing utilities.

2. Place the handhole in its intended hole as soon as the hole is dug. Set at 1 inch below grade from the top of handhole. No holes can be left open for an extended period, as determined by the Engineer.

3. Open handholes along existing segments of conduit, where power and communication cables are, or will be, co-located.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Hh, Round, Commun Each

**Hh, Round, Commun** includes constructing a round handhole and providing hardware, connectors, fittings, and all material necessary to complete the work.