MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**CONCRETE, GRADE 6000HP**

CFS:CRB 1 of 1 APPR:JAB:TES:09-20-23

**a. Description.** This work consists of providing PCC, Grade 6000HP. Perform all work in accordance with the contract, except as modified herein.

**b. Materials.** Furnish materials in accordance with section 1004 of the Standard Specifications for Construction for Concrete 4500HP, except the minimum 28-day compressive strength is 6,000 psi.

**c. Construction.** Ensure construction methods are in accordance with subsection 706.03 of the Standard Specifications for Construction.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Conc, Grade 6000HP Cubic Yard

**Conc, Grade 6000HP** includes all necessary labor, equipment, and materials to furnish, form, place, finish, and cure PCC, Grade 6000HP and will be measured and paid for in accordance with subsection 706.04 of the Standard Specifications for Construction.