MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**BRIDGE BARRIER RAILING, AESTHETIC, TYPE 6, DET\_\_, HIGH PERFORMANCE, MODIFIED**

BRG:CFO 1 of 1 APPRSCK:NAP:03-30-22

**a. Description.** This work consists of constructing bridge railing in accordance with section 711 of the Standard Specifications for Construction, the plans, and as specified herein.

**b. Materials.** Furnish materials in accordance with subsection 711.02 of the Standard Specifications for Construction.

**c. Construction.** Construct bridge railings in accordance with subsection 711.03 of the Standard Specifications for Construction, as shown on the plans and this special provision.

1. Construct the length of barrier from MDOT Special Detail B-29-A, Section A-A.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Bridge Barrier Railing, Aesthetic, Type 6, Det\_\_, High Performance, Modified Foot

**Bridge Barrier Railing, Aesthetic, Type 6, Det \_\_, High Performance, Modified** will be measured based on plan quantities. **Bridge Barrier Railing, Aesthetic, Type 6, Det \_\_, High Performance, Modified** includes providing and placing concrete, constructing joints, forming, finishing, curing, and protecting the concrete, placing light standard anchor bolt assemblies, concrete that fills form liners and concrete necessary to construct the railing to the shape shown on the plans.

Furnishing reinforcing steel will be paid for as specified in subsection 706.04 of the Standard Specifications for Construction.