MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**TRAFFIC SIGNAL MAST ARMS AND POLES, ROAD COMMISSION FOR OAKLAND COUNTY FURNISHED**

SIG:JYP 1 of 1 APPR:EMS:DBP:03-28-23

**a. Description.** This work consists of picking up, transporting and erection of new traffic signal mast arms and poles as shown on the plans, in accordance with the standard specifications and this special provision. The Road Commission for Oakland County will furnish the traffic signal mast arms and poles. Pick up the traffic signal mast arms and poles at:

Road Commission for Oakland County

2420 Pontiac Lake Road

Waterford, MI 48328

Contact: Danielle Deneau

Phone: 248-858-4802

Contact Danielle Deneau, PE, Director of Traffic-Safety at 248-858-4802, 1 week in advance of the desired pick up date. Transport the traffic signal mast arms and poles to the job site for installation.

**b. Erection.** Verify the anchor bolt arrangement and proper template with the furnished traffic signal mast arm poles prior to construction of the foundation. Anchor bolts will not be paid for separately but are included in the payment for the signal pole foundations. Place and tighten nuts and washers on anchor bolts in accordance with subsection 810.03.N of the Standard Specifications for Construction. Ensure all installation procedures are witness by the Engineer.

**c. Construction.** Ensure all construction is in accordance with sections 818 and 820 and subsection 810.03 of the Standard Specifications for Construction, as shown on the plans and as directed by the Engineer.

Repair coating damaged in transporting, handling, or erection in accordance with subsection 716.03.E of the Standard Specifications for Construction at no additional cost to the Department.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Mast Arm, \_\_foot, Cat I, County Furn Each

Mast Arm Pole, Cat I, Anchor Base, County Furn Each

1. **Mast Arm, \_\_ foot, Cat I, County Furn**, includes pickup, transport, and erection on **Mast Arm Pole, Cat I, Anchor Base, County Furn** and associated hardware.

2. **Mast Arm Pole, Cat I, Anchor Base, County Furn**, includes pickup, transport, and erection on Mast Arm Pole Fdn, 6 Bolt.