MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**MOVEABLE BARRIER WALL LAYOUT LINE**

NOR:DWM 1 of 1 APPR:CRB:MRB:02-15-22

**a. Description.** This work consists of placing temporary pavement markings for the layout of moveable barrier wall at locations specified on the plans, in accordance with the standard specifications, and as specified herein.

**b. Materials.** Ensure materials meet the requirements of sections 812.02 and 922 of the Standard Specifications for Construction except that there are no retroreflectivity requirements. Other material may be allowed but requires prior approval by the Engineer. Ensure the color is white unless otherwise approved by the Engineer.

**c. Construction.** Ensure construction methods meet the requirements of section 812.03.D.12 of the Standard Specifications for Construction except as modified herein. Place two-foot-long dashes at maximum one-inch width spaced four feet apart from center-to-center of the markings unless otherwise approved by the Engineer. This is only to be used to provide a layout line for the planned movement of the moveable barrier wall.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for in accordance with section 812.04 at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Moveable Wall Layout Line Temp Foot