MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**AGGREGATE, SPECIAL**

BRG:MGB 1 of 1 APPR:DMG:JFS:05-19-21

**a. Description.** This work consists of furnishing and placing aggregate within the void space of riprap inside and outside of culverts as shown on the plans.

**b. Materials.** Furnish materials in accordance with Tables 902-1 and 902-2 of the Standard Specifications for Construction for open-graded drainage course Class 46G.

**c. Construction.** Place aggregate within the riprap void space to the depth shown on the plans. Place aggregate in accordance with subsection 206.03.B of the Standard Specifications for Construction, as shown on the plans and detailed herein. Density requirements are waived.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Aggregate, Spec Cubic Yard

**Aggregate, Spec** will be measured by volume, loose measure. The unit price for **Aggregate, Spec** includes furnishing, hauling, and placing the material at the locations shown on the plans.