MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**BICYCLE LANE SEPARATORS**

OAK:LLS 1 of 1 APPR:MWB:MKB:06-28-22

**a. Description.** This work consists of furnishing and installing lane separators as shown on the plans and as directed by the Engineer. Construct lane separators in accordance with the plans and in accordance with the requirements of section 810 of the Standard Specifications for Construction except as modified herein.

**b. Materials.** Furnish lane separators and related components selected and approved by the City of Pleasant Ridge. Use tools and equipment as recommended by the manufacturer and as approved by the Engineer.

Ensure the lane separators and related components are Zicla Zebra Cycle Lane Separators as manufactured by: Transline Industries, Grand Prairie, TX. (972) 647-8300. sales@translineinc.com.

1. Lane Separator.

A. Color - White

B. Size - 9

2. Anchors.

A. Size - 15 cm length; 16 mm diameter

**c. Construction.** Secure lane separators to the roadway with removable and reusable threaded rods, M12 hex nuts, and styrene-free epoxy resin per manufacturer’s requirements. Lane separator system system to be completely removable and replaceable with standard tools.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Bicycle Lane Separator Each