[MICHIGAN](http://mdotcf.state.mi.us/public/design/englishroadmanual/)

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**AGGREGATE, 4AA**

MET:RDM 1 of 1 APPR:DMG:TEB:04-29-21

**a. Description.** This work consists of providing and placing coarse aggregate within an excavated trench for the infiltration storage.

**b. Materials.** Furnish Class 4AA coarse aggregate in accordance with section 902 of the Standard Specifications for Construction with the following exceptions:

1. Ensure aggregate provided is natural aggregate only, free of cementitious materials and associated detritus.

2. Wash aggregate and ensure it is free of all fines at the time of final placement.

**c. Construction.** Place Class 4AA coarse aggregate to the limits shown on the plans and as directed by the Engineer. Compaction will not be tested.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Aggregate, 4AA Cubic Yard

**Aggregate, 4AA** will be measured by volume, loose measure. Payment for **Aggregate, 4AA** constitutes full compensation for completing the work as described herein including the cost of providing, hauling and placing material.