MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**EXISTING NOISE WALL PANELS, REMOVE AND RE-ERECT**

MAC:SNK 1 of 1 APPR:JAB:DMG:06-12-25

**a. Description.** This work consists of removing, salvaging, protecting, and re-erecting existing noise wall panels at the locations shown on the plans.

**b. Materials.** Furnish all materials required for removing and re-erecting the noise wall panels in accordance with section 907 of the Standard Specifications for Construction.

**c. Construction.** Prior to the removal, inspect existing noise wall panels and report any damage to the Engineer. Replace any panel that, in the opinion of the Engineer, has been damaged or otherwise rendered useless by the improper storage or handling at no cost to the contract. Salvage and store the removed panels in a secured area within the Department’s right-of-way. Protect the panels from weather and accidental damage. Re-erect panels after the concrete surface coating has been applied to the supporting barriers.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Existing Noise Wall Panels, Rem and Re-Erect Foot

**Existing Noise Wall Panels, Rem and Re-Erect** includes all labor, equipment, materials and transportation required for removal, salvaging, storage, and re-erection of the noise wall panels as described in this special provision.