MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**PAVEMENT REMOVAL, MODIFIED**

DET:ALW 1 of 1 APPR:DMG:DBP:06-28-24

**a. Description.** This work consists of removing existing HMA pavement, reinforced or non-reinforced concrete pavement, brick pavers, curb, and curb and gutter to the limits shown on the plans regardless of the existing material type or number of layers and thickness of individual layers.

**b. Materials.** Furnish materials in accordance with subsection 204.02 of the Standard Specifications for Construction.

**c. Construction.** Remove and dispose of existing HMA pavement, reinforced or non-reinforced concrete pavement, curb, curb and gutter, and brick pavers in accordance with subsection 204.03 of the Standard Specifications for Construction. Take care not to chip, break, or otherwise damage existing brick pavers during removal. Salvage pavers for reuse on site in accordance with the plans as directed by the Engineer. Ensure pavers that are determined by the Engineer to have been damaged during removal or excess pavers are properly disposed of upon completion of salvaging.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Pavt, Rem, Modified Square Yard

**Pavt, Rem, Modified** will be measured and paid for once for all areas identified for removal, regardless of the existing material type, number of layers or thickness of individual layers. Track removal will be paid for separately. Salvaging brick pavers will be paid for separately.