MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**PAVILION COLUMN WRAP**

OAK:KHC 1 of 1 APPR:BMB:NJM:05-23-24

**a. Description.** This work consists of furnishing and installing pavilion column wrap as shown on the plans. This work includes an electrical outlet package required for a complete installation.

**b. Materials.**

1. Stone Veneer Package. Furnish precast concrete mortarless stone veneer and capstone, resembling natural stone in both texture and color manufactured by Ply Gem Residential Solutions as Clipstone ColumnWrap or Engineer-approved equal. Ensure each veneer unit has galvanized metal mounting clips and is engineered to resist the effects of weathering. Ensure style and color are Northern Ledge Niagara.

2. Electrical Outlet Package. Furnish materials in accordance with section 918 of the Standard Specifications for Construction and the requirements of this special provision.

A. Furnish 20-ampere Ground-Fault Circuit Interrupters (GFCI) receptacle protected by an upstream circuit breaker.

B. Furnish a single-gang, vandal-resistant, in-use cover plate with locking mechanism by Vandal Stop, Red Dot, or Engineer-approved equal.

**c. Construction.** Install pavilion column wrap in accordance with manufacturer’s specifications and instructions, section 818 of the Standard Specifications for Construction, as shown on the plans, and this special provision.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay items:

**Pay Item Pay Unit**

Stone Veneer Package Each

Electrical Outlet Package Each

Electrical wiring and conduit to the electrical outlet will be paid for separately.