MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**PICNIC TABLE**

OAK:KHC 1 of 1 APPR:YGQ:JG:05-22-24

**a. Description.** This work consists of furnishing and installing a freestanding recycled slat picnic table in accordance with the details and at the location shown on the plans.

**b. Materials.** Furnish picnic table materials selected and approved by the Engineer. Acceptable manufacturers and styles of picnic tables are as follows.

1. Picnic table. Furnish fabricated metal components that are steel shot blasted, etched, phosphatized, preheated, and electrostatically powder-coated with triglycidyl isocyanurate (TGIC) polyester powder coatings or approved equal. Use recycled plastic slats. The final color will be selected by the Engineer from the manufacturer’s samples.

A. Picnic Table, 6 foot. Standard 6 foot length table and two backless benches.

B. Picnic Table, 8 foot. ADA-compliant pair table in extended 8 foot length with 6 foot two backless benches.

C. Select picnic table from one of the following Manufacturers or Engineer approved equal:

Product Name Supplier Telephone No.

NRB-6, CM-565 Victor Stanley, LLC. (800) 368-2573

NY6-1500-RP, NY6-2500-ADA-RP SiteScapes, Inc. (888) 331-9464

**c. Construction.** Assemble picnic table in accordance with manufacturer’s instructions. Install picnic table level and square in a true, flat plane to prevent rocking.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay items:

**Pay Item** **Pay Unit**

Picnic Table, 6 foot Each

Picnic Table, 8 foot Each