MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIFICATION

FOR

**REFLECTIVE PANEL FOR PERMANENT SIGN SUPPORT, MODIFIED**

NOR:KLM 1 of 1 APPR:GJD:AJU:08-13-24

**a. Description.** This work consists of furnishing, fabricating, and erecting a reflective panel to sign supports in accordance with section 810 of the Standard Specifications for Construction, as shown on the plans and as specified herein.

**b. Materials.** Furnish and fabricate all components, hardware, and other appurtenances in accordance with section 919 of the Standard Specifications of Construction except as modified by this special provision.

Delete the third paragraph of subsection 919.02.B.5 and replace with the following:

“Attach the reflective strip to 0.080-inch-thick aluminum substrate. If used on a u-channel post, a backing plate is required.”

**c. Construction.** Complete this work in accordance with sections 810.03 of the Standard Specifications for Construction and as directed by the Engineer.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Reflective Panel for Permanent Sign Support, \_\_ foot, Modified Each