MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**ASH URN**

RSD:NMA 1 of 1 APPR:JN:MJF:04-04-23

**a. Description.** This work consists of furnishing in place a pre-cast concrete ash urn as described in this special provision at locations shown on the plans.

**b. Materials.** Pre-cast concrete 14 inches square, by 24 inches high, by 11 inches square at the chamfered base with acid wash stain, charcoal color. Reinforce the container with 1/4 inch diameter steel rebar, and use grade 3500 concrete in accordance with the standard specifications.

**c. Shop Drawings.** Submit complete shop drawings for this item in PDF that requires Engineer review and approval. Manufacture the ash urns after Engineer approves shop drawings.

**d. Construction.** Place pre-cast concrete ash urns as shown on the plans and as directed by the Engineer.

**e.** **Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item.

**Pay Item Pay Unit**

Ash Urn Each