MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**EXISTING SIDEWALK, CLEAN AND EDGE**

DET:ALW 1 of 1 APPR:DMG:TEB:10-05-21

**a. Description.** This work consists of removing accumulated earth, vegetation and debris from the surface, joints and cracks of existing sidewalks and curb ramps, including the joints between these facilities and adjacent curb, curb and gutter, and roadway and driveway pavements, to reduce potential hazards to pedestrian traffic. It also includes edging of existing sidewalks and curb ramps to restore the originally constructed usable width of these facilities.

**b. Materials.** None specified.

**c. Construction.** Furnish shovels, hand edgers, hand brooms, power edgers, power brooms, air compressors, water-flushing equipment, and other equipment needed to perform the work.

Clean and edge existing sidewalks and curb ramps by completely removing accumulated earth, vegetation, and debris flush to the existing surface without marring or damaging these surfaces, detectable warning surfaces or adjacent curb, curb and gutter and pavement surfaces. Ensure damage caused by the Contractor’s operation as determined by the Engineer is repaired at no cost to the contract.

Dispose of the removed materials in accordance with subsection 205.03.P of the Standard Specifications for Construction.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Existing Sidewalk, Clean and Edge Square Foot

**Existing Sidewalk, Clean and Edge** will be measured and paid for by the area of existing sidewalk and curb ramps cleaned and edged and includes the disposal of removed materials.

If after cleaning and edging the Engineer determines that deterioration or damage not caused by the Contractor’s operation must be repaired, such work will be measured and paid for separately.