MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**BICYCLE LANE DELINEATOR POST**

DET:ALW 1 of 1 APPR:MWB:MKB:11-04-21

**a. Description.** This work consists of furnishing and installing delineator posts as shown on the plans and as directed by the Engineer. Construct delineators in accordance with the plans and in accordance with the requirements of section 810 of the Standard Specifications for Construction except as modified herein.

**b. Materials.** Furnish delineator posts and related components selected and approved by the City of Detroit. Use tools and equipment as recommended by the manufacturer and as approved by the Engineer.

Ensure the delineator post and related components are FG 300 Model EFX Channelizer Post as manufactured by: Pexco LLC - Davidson Traffic Control Products, Tacoma, WA. (877) 335-4638. [hwysales@pexco.com](mailto:hwysales@pexco.com)

1. Delineator Post.

A. Color - White

B. Height - 36 inches

2. Delineator Base.

A. Color - White

3. Reflective Sheeting.

A. Color - White

B. Two 6-inch wide wraps

**c. Construction.** Secure delineator posts to the roadway with removable and reusable one-piece anchor bolts with a finished hex-head, integral washer, dual lead threads and chamfered tip per manufacturer’s requirements. Use one-piece bolts to eliminate improper assembly and use dual-thread bolts to prevent bolts spinning in holes when tightened. Delineator post system to be completely removable and replaceable with standard power tools.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Post, Delineator, 36 inch, White Each