MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**AGGREGATE BASE, \_\_ 21AA, MODIFIED**

OFS:MH 1 of 1 APPR:SAG:DMG:11-26-24

**a. Description.** This work consists of the manufacture of the aggregate base shown on the plans from crushed limestone as described in this special provision and placed on a suitable subgrade as determined by the Engineer. Ensure all work is completed in accordance with section 302 of the Standard Specifications for Construction, except as specified herein.

**b. Materials.** Ensure material is accordance with Tables 902-1 and 902-2 of the Standard Specifications for Construction for gradation and physical requirements for dense-graded aggregate Class 21AA.

**c. Construction.** Complete all work in accordance with the standard specifications.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Aggregate Base, \_\_ inch, 21AA, Modified Square Yard

**Aggregate Base, \_\_ inch, 21AA, Modified** includes all labor, equipment, and materials required to complete the work described.