MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**BIKE RACK**

DET:ALW 1 of 1 APPR:YGQ:JLG:08-26-24

**a. Description.** This work consists of placing bike racks in the areas shown on the plans. Perform all work in accordance with sections 815 and 816 of the Standard Specifications for Construction.

**b. Materials.** Furnish steel tube bike rack(s) with surface mounting. Ensure bike rack(s) are one of the following or an approved equal:

Model/Manufacturer

● U2 Series/CycleSafe, Grand Rapids, MI 49546, (888) 950-6531

● Sonance One Loop/Keystone Ridge Designs, Butler, PA 16001, (800) 284-8208

**c. Preparation.** Coordinate this work with the Engineer before construction to establish locations and review proposed installation methods. Electronically submit a complete set of shop drawings for this item to the Engineer within 7 days of award. The Engineer will review and approve or reject the shop drawings within 14 days of receipt. The approval of shop drawings does not relieve the Contractor from the responsibility to correct errors or omissions and to comply with 20SP105A - Source of Steel and Iron (Buy America).

**d. Construction.** Install the bike racks as shown on the plans and per the manufacturer’s specifications and recommendations. Surface mount installation is required. Identify each part prior to assembly. Tighten all bolts, nuts, and fasteners only after final adjustment and leveling permanently. Use construction methods in accordance with section 803 of the Standard Specification for Construction unless otherwise stated in this special provision.

**e. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Bike Rack Each

**Bike Rack** includes surface mounting of the bike rack as shown on the plans and per manufacturer’s specifications and recommendations as required for installation.