MICHIGAN

DEPARTMENT OF TRANSPORTATION

SPECIAL PROVISION

FOR

**SANITARY SEWER SERVICE LEAD CONFLICT**

BCY:DJM 1 of 1 APPR:RPB:CJD:01-31-24

**a. Description.** This work consists of relocating (lowering) existing sanitary sewer service leads that conflict with proposed storm sewer or water main installation where called for on the plans or where directed by the Engineer.

**b. Materials.** Furnish materials in accordance with section 825 of the Standard Specifications for Construction, the City of Saginaw, and as called for in the details on the plans. Confirm the type of existing sanitary sewer service materials and type of adaptors needed to connect to existing sanitary sewer service in the field. Ensure fittings, solvents, lubricants, and cements for the joining of pipes are as recommended by the pipe manufacturer.

**c. Construction.** Perform the sanitary sewer service relocation work in accordance with section 825 of the Standard Specifications for Construction, the requirements of the details on the plans and the City of Saginaw standards. Make pipe connections as recommended by the pipe manufacturer.

The City of Saginaw will be responsible for shutting down the wastewater system to facilitate relocation of the sanitary sewer service. Contact the City of Saginaw a minimum of 3 full working days prior to construction to enable the work to be scheduled. Coordinate the work with the City of Saginaw.

**d. Measurement and Payment.** The completed work, as described, will be measured and paid for at the contract unit price using the following pay item:

**Pay Item Pay Unit**

Sanitary Sewer, Serv Lead, Conflict Each

**Sanitary Sewer, Serv Lead,** **Conflict** includes payment in full for furnishing all materials including wyes, miscellaneous fittings, pipe, dewatering, bracing or sheeting, blocking, and all other miscellaneous items, labor, and equipment necessary to perform the work specified herein and as shown on the plans.

Earth excavation and backfilling, together with any related work encountered, unless otherwise specified, will be considered as included in **Sanitary Sewer, Serv Lead, Conflict**.